Saving Router Configurations

|  |  |
| --- | --- |
| Command | Description |
| **configure terminal** | enters global configuration mode from privileged EXEC mode |
| **copy running-config** **startup-config** | saves the configuration file |
| **enable** | enters privileged EXEC mode |
| **erase startup-config** | deletes the startup configuration file in non-volatile random access memory (NVRAM) |
| **exit** | exits one level in the menu structure |
| **hostname** *host-name* | sets the device name |
| **reload** | Reboots the Router |
| **show running-config** | displays the active configuration file |
| **show startup-config** | displays the backup configuration file |